
;
;----------------------------------------------------------------------------------------------------------------------
; mdmsiewm.inf
; version 2.6
; Date 2003/02/20
;
; „nderung von 2.4 zu 2.6:    HKR, Init,1,, "AT&F&D2&C1E0V1S0=0<cr>"
;   HKR, Settings, DialSuffix,, ""
;   HKR, Settings, Pulse,, "P"
;   HKR, Settings, Tone,, "T"
;   HKR,, Properties, 1, 00,00,00,00, 3C,00,00,00, 00,00,00,00, ...
;   MC388 --> 230kbps
;
;
; Siemens - Wireless Modules ----- GSM/GPRS devices ----- modem function installation
;
; Author: Markus Enck - ICM WM AE SL
;         Marten Petschke - ICM WM AE CS
;         Wohler Martin - ICM WM RD
;
; Copyright (c) 2003, Siemens AG
;----------------------------------------------------------------------------------------------------------------------
;


[Version]
LayoutFile=mdmsiewm_v2.6.inf
Signature="$CHICAGO$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Mfg%
DriverVer=02/20/2003

[Manufacturer]
; The string below will appear in the Install New Modem wizard's list of manufacturers
%Mfg% = Models

[Models]
; This list will appear in the Install New Modem wizard's list of modems
%Modem1%  = Modem1,   MC35      ; "MC35 (GPRS)"
%Modem6%  = Modem6,   MC45      ; "MC45 (GPRS)"
%Modem7%  = Modem7,   TC35      ; "TC35"
%Modem9%  = Modem9,   MC388     ; "MC388 (GPRS)"
%Modem10% = Modem10,  AC35      ; "AC35 (GPRS)"
%Modem11% = Modem11,  AC45      ; "AC45 (GPRS)"



[Strings]
; This section lists strings that are used by the Modems control panel applet
; and the Install New Modem wizard.
Mfg    = "Siemens AG - Wireless Modules"
Modem1   = "MC35 (GPRS)"
Modem6   = "MC45 (GPRS)"
Modem7   = "TC35"
Modem9   = "MC388 (GPRS)"
Modem10  = "AC35 (GPRS)"
Modem11  = "AC45 (GPRS)"




[Modem1.ntx86]
AddReg=W2KPat.AddReg, All, External, GSM_PROTOCOL2, FAXCLASS, VerboseResultCodes, SIEMENS2.AddReg

[Modem1]
AddReg=All, External, VerboseResultCodes, GSM_PROTOCOL2, FAXCLASS, SIEMENS2.AddReg


[Modem6.ntx86]
AddReg=W2KPat.AddReg, All, External, VerboseResultCodes,GSM_PROTOCOL2, FAXCLASS, SIEMENS3.AddReg

[Modem6]
AddReg=All, External, VerboseResultCodes, GSM_PROTOCOL2, FAXCLASS, SIEMENS3.AddReg


[Modem7.ntx86]
AddReg=W2KPat.AddReg, All, External, VerboseResultCodes, GSM_PROTOCOL1, FAXCLASS, SIEMENS1.AddReg

[Modem7]
AddReg=All, External, VerboseResultCodes, GSM_PROTOCOL1, FAXCLASS, SIEMENS1.AddReg


[Modem9.ntx86]
AddReg=W2KPat.AddReg, All, External, VerboseResultCodes, GSM_PROTOCOL2, FAXCLASS, SIEMENS3.AddReg

[Modem9]
AddReg=All, External, VerboseResultCodes, GSM_PROTOCOL2, FAXCLASS, SIEMENS3.AddReg


[Modem10.ntx86]
AddReg=W2KPat.AddReg, All, External, VerboseResultCodes, GSM_PROTOCOL2, FAXCLASS, SIEMENS2.AddReg

[Modem10]
AddReg=All, External, VerboseResultCodes, GSM_PROTOCOL2, FAXCLASS, SIEMENS2.AddReg


[Modem11.ntx86]
AddReg=W2KPat.AddReg, All, External, VerboseResultCodes, GSM_PROTOCOL2, FAXCLASS, SIEMENS2.AddReg

[Modem11]
AddReg=All, External, VerboseResultCodes, GSM_PROTOCOL2, FAXCLASS, SIEMENS2.AddReg



[All]

HKR,,FriendlyDriver,,unimodem.vxd
HKR,,DevLoader,,*vcomm
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init,      1,, "AT&F&D2&C1E0V1S0=0<cr>"
HKR, Monitor,   1,, "ATS0=0<cr>"
HKR, Monitor,   2,, "None"
HKR, Hangup,    1,, "ATH<cr>"
HKR, Answer,    1,, "ATA<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, FlowControl_Off,,  "\Q0"
HKR, Settings, FlowControl_Hard,, "\Q3"
HKR, Settings, FlowControl_Soft,, "\Q1"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"


[EXTERNAL]
HKR,, DeviceType, 1, 01

[GSM_PROTOCOL1]
HKR, Protocol\GSM\ANALOG_RLP, 1,,"AT+CBST=0,0,1<cr>"
HKR, Protocol\GSM\V110_2DOT4K, 1,,"AT+CBST=68,0,1<cr>"
HKR, Protocol\GSM\V110_4DOT8K, 1,,"AT+CBST=70,0,1<cr>"
HKR, Protocol\GSM\V110_9DOT6K, 1,,"AT+CBST=71,0,1<cr>"
HKR, Protocol\GSM\V110_14DOT4K, 1,,"AT+CBST=75,0,1<cr>"


[GSM_PROTOCOL2]
HKR, Protocol\GSM\ANALOG_RLP, 1,,"AT+CBST=0,0,1<cr>"
HKR, Protocol\GSM\V110_2DOT4K, 1,,"AT+CBST=68,0,1<cr>"
HKR, Protocol\GSM\V110_4DOT8K, 1,,"AT+CBST=70,0,1<cr>"
HKR, Protocol\GSM\V110_9DOT6K, 1,,"AT+CBST=71,0,1<cr>"
HKR, Protocol\GSM\V110_14DOT4K, 1,,"AT+CBST=75,0,1<cr>"
HKR, Protocol\GSM\GPRS, 1,,"AT<cr>"

[FAXCLASS]
HKR, Fax, ResetCommand,, "ATE0V1Q0"
HKR,, FClass, 1, 0B,00,00,00
HKR, Fax, Class1DTESpeed,, "AUTO"
HKR, Fax, FixModemClass,, "2"
HKR, Fax, FixSerialSpeed,,"19200"
HKR, Fax, SerialSpeedInit,, "19200"
HKR, Fax\Class1\AdaptiveAnswer, SerialSpeedFaxDetect,, "19200"


[VerboseResultCodes]
HKR, Responses, "<cr><lf>OK<cr><lf>",          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+CRING: FAX<cr><lf>", 1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+CRING: REL ASYNC<cr><lf>", 1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",  1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",   1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",     1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "0<cr>", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "1<cr>", 1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "2<cr>", 1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "3<cr>", 1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "4<cr>", 1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "6<cr>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "7<cr>", 1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "8<cr>", 1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "10<cr>", 1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "30<cr>", 1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "32<cr>", 1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "47<cr>", 1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "48<cr>", 1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "49<cr>", 1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "33<cr>", 1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "50<cr>", 1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",         1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",    1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",    1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",    1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>",   1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800<cr><lf>",   1, 02, 00, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",   1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600<cr><lf>",   1, 02, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000<cr><lf>",   1, 02, 00, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400<cr><lf>",   1, 02, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>",   1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",   1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",   1, 02, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",  1, 02, 00, 00,C2,01,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 2400/RLP<cr><lf>",    1, 02, 00, 60,09,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 4800/RLP<cr><lf>",    1, 02, 00, C0,12,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/RLP<cr><lf>",    1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/RLP<cr><lf>",   1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 16800/RLP<cr><lf>",   1, 02, 00, A0,41,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/RLP<cr><lf>",   1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 21600/RLP<cr><lf>",   1, 02, 00, 60,54,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 24000/RLP<cr><lf>",   1, 02, 00, C0,5D,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 26400/RLP<cr><lf>",   1, 02, 00, 20,67,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/RLP<cr><lf>",   1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/RLP<cr><lf>",   1, 02, 00, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/RLP<cr><lf>",   1, 02, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 115200/RLP<cr><lf>",  1, 02, 00, 00,C2,01,00, 00,00,00,00



; TCxx devices with 19200bps, 8n1 as default com port settings, additinal the Xon/Xoff configuration is defined
[SIEMENS1.AddReg]
HKR,, Properties, 1, 80,01,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 10,01,00,00, 00,c2,01,00, 00,4b,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,4B,00,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,, ConfigDelay, 1, b8,0b,00,00

; MCxx devices with 115200bps, 8n1 as default com port settings, additinal the Xon/Xoff configuration is defined
[SIEMENS2.AddReg]
HKR,, Properties, 1, 00,00,00,00, 3C,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 30,00,00,00, 00,C2,01,00, 00,C2,01,00
HKR,, ConfigDelay, 1, b8,0b,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,C2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00


; MC45  devices with 230400bps, 8n1 as default com port settings, additinal the Xon/Xoff configuration is defined
[SIEMENS3.AddReg]
HKR,, Properties, 1, 00,00,00,00, 3C,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 30,00,00,00, 00,84,03,00, 00,C2,01,00
HKR,, ConfigDelay, 1, b8,0b,00,00
HKR,, DCB, 1, 1C,00,00,00, 00,C2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

;Indicates the number of Configure-Request packets sent without receiving a valid Configure-Ack, Configure-Nak
;or Configure-Reject before assuming that the peer is unable to respond
[W2KPat.AddReg]
HKLM,"SYSTEM\CurrentControlSet\Services\RasMan\PPP",MaxConfigure,0x00010001,50

